(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(BT1-+)")
  (net 2 "Net-(BT1--)")
  (net 3 "Net-(U1A-THR)")
  (net 4 "Net-(U1B-DIS)")
  (net 5 "Net-(U1B-Q)")
  (net 6 "/Output")
  (net 7 "Net-(D1-A)")
  (net 8 "Net-(SW1-B)")
  (net 9 "Net-(U1A-DIS)")
  (net 10 "Net-(R3-Pad1)")
  (net 11 "Net-(R4-Pad1)")
  (net 12 "unconnected-(U1A-CV-Pad3)")
  (net 13 "Net-(U1A-Q)")
  (net 14 "unconnected-(U1B-CV-Pad11)")

  (footprint "Capacitor_THT:CP_Radial_D8.0mm_P5.00mm" (layer "F.Cu")
    (tstamp 31368880-1267-4941-a5e9-5357d2a2f160)
    (at 168 83)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=8mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 8mm Electrolytic Capacitor")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (path "/4d86dd88-5876-4541-bd99-b3a653e81f9a")
    (attr through_hole)
    (fp_text reference "C3" (at 2.5 -5.25) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f3efc0fb-bbde-4ce9-9215-f0c3800fb85e)
    )
    (fp_text value "10uF" (at 2.5 5.25) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2302f98c-53a7-453d-b17b-791aef3152f4)
    )
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f97a1111-1135-4fc1-bbaa-1e135bc9e652)
    )
    (fp_line (start -1.909698 -2.315) (end -1.109698 -2.315)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 779a4653-848d-47ca-939a-9c6995de2727))
    (fp_line (start -1.509698 -2.715) (end -1.509698 -1.915)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0552b721-cfe1-4386-bc6b-4971b2b8eca3))
    (fp_line (start 2.5 -4.08) (end 2.5 4.08)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp facc0d9f-6c37-45cf-b97d-ea7034d1f34a))
    (fp_line (start 2.54 -4.08) (end 2.54 4.08)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e204453f-f693-424e-8a1f-84ae07706d09))
    (fp_line (start 2.58 -4.08) (end 2.58 4.08)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ed21e5e7-ffa9-4dea-a52b-0e899a1be466))
    (fp_line (start 2.62 -4.079) (end 2.62 4.079)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f8c63d78-2c14-42b9-abbf-a5383fee2860))
    (fp_line (start 2.66 -4.077) (end 2.66 4.077)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ba38edc4-0735-43f4-9313-e0d3e13cb960))
    (fp_line (start 2.7 -4.076) (end 2.7 4.076)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 377793a8-ca0d-4a72-a751-6cc1b2bc3d65))
    (fp_line (start 2.74 -4.074) (end 2.74 4.074)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e57f13d-61d7-4e26-8d68-7afdf41642a9))
    (fp_line (start 2.78 -4.071) (end 2.78 4.071)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bc7a66c7-40af-4be5-8871-cc5959de29a1))
    (fp_line (start 2.82 -4.068) (end 2.82 4.068)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 102092c9-0641-4fe6-a5c7-4ec9375bcd08))
    (fp_line (start 2.86 -4.065) (end 2.86 4.065)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f387cb37-6f16-45d9-b019-07ad1828d900))
    (fp_line (start 2.9 -4.061) (end 2.9 4.061)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bf9790c3-6e53-4f71-a0c8-61a611de8ab7))
    (fp_line (start 2.94 -4.057) (end 2.94 4.057)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 036f78a2-bee0-4939-939a-a7ca96e41aa6))
    (fp_line (start 2.98 -4.052) (end 2.98 4.052)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d1a949c9-bc0a-4026-9660-7ddad2ae40bc))
    (fp_line (start 3.02 -4.048) (end 3.02 4.048)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7cfc4c3f-ae76-4257-be80-9656a6f064b0))
    (fp_line (start 3.06 -4.042) (end 3.06 4.042)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3212d0fd-4a13-4a8d-8f6e-61428a6a2fbf))
    (fp_line (start 3.1 -4.037) (end 3.1 4.037)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp be258b05-8414-4dab-9258-3442ffe80078))
    (fp_line (start 3.14 -4.03) (end 3.14 4.03)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2f28384e-e726-404e-9ced-939052476688))
    (fp_line (start 3.18 -4.024) (end 3.18 4.024)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7c397cbe-9908-49d0-aba7-fb273c992873))
    (fp_line (start 3.221 -4.017) (end 3.221 4.017)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0cd3848b-cd0f-40fb-b93d-2cdea2c82d67))
    (fp_line (start 3.261 -4.01) (end 3.261 4.01)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1527b94e-9c8c-4705-ad8e-c7e1cf6baa95))
    (fp_line (start 3.301 -4.002) (end 3.301 4.002)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4487ec02-c5b2-4463-89c3-551a398ed0dc))
    (fp_line (start 3.341 -3.994) (end 3.341 3.994)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1cde6a0d-239e-4908-8e67-e00cd3c509bc))
    (fp_line (start 3.381 -3.985) (end 3.381 3.985)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ee043f99-4021-4400-ba68-f7c2ae7d0a58))
    (fp_line (start 3.421 -3.976) (end 3.421 3.976)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2c0d1b58-fcde-4b97-921a-148d8da51d6f))
    (fp_line (start 3.461 -3.967) (end 3.461 3.967)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 930d27e2-5731-49d4-94e7-da3f291d8b23))
    (fp_line (start 3.501 -3.957) (end 3.501 3.957)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 385bc4c4-ba15-4eab-9fa2-71df3f229cf2))
    (fp_line (start 3.541 -3.947) (end 3.541 3.947)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 23b3f3bf-57c6-4fac-92ad-b5dbc5eb5b90))
    (fp_line (start 3.581 -3.936) (end 3.581 3.936)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1ab189a9-4e51-4215-93be-fb11d043ddd1))
    (fp_line (start 3.621 -3.925) (end 3.621 3.925)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e921f2b-fcaf-412d-b66a-4273d728cfb2))
    (fp_line (start 3.661 -3.914) (end 3.661 3.914)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 943ef6ce-ef37-454d-9fe9-73ae85f3dced))
    (fp_line (start 3.701 -3.902) (end 3.701 3.902)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c81f78e5-c806-450e-9e6a-026125e690ad))
    (fp_line (start 3.741 -3.889) (end 3.741 3.889)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6c0261ea-b7f0-4d2f-84ab-0ff10e989ad8))
    (fp_line (start 3.781 -3.877) (end 3.781 3.877)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d665d86e-5d54-4019-a621-30b2d0d12f33))
    (fp_line (start 3.821 -3.863) (end 3.821 3.863)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eb62fef8-268a-4502-a9bc-4625c0aebbd6))
    (fp_line (start 3.861 -3.85) (end 3.861 3.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5bb755c4-4a4e-41d3-8cf4-c3055fedcb14))
    (fp_line (start 3.901 -3.835) (end 3.901 3.835)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e5b6769c-b0fd-4e83-8c0e-1ddcdd2b8573))
    (fp_line (start 3.941 -3.821) (end 3.941 3.821)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp de5df046-0cdf-4614-8b83-7286ad0e9cb4))
    (fp_line (start 3.981 -3.805) (end 3.981 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 72f8f350-5992-458b-a40b-051c2550d88f))
    (fp_line (start 3.981 1.04) (end 3.981 3.805)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 58efd2d8-d452-46a0-9c57-14ffe6c71a23))
    (fp_line (start 4.021 -3.79) (end 4.021 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6c0512f9-abe6-4d26-805d-913f4fc318c5))
    (fp_line (start 4.021 1.04) (end 4.021 3.79)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 986e0151-ac59-48d9-a92f-5cde29088c05))
    (fp_line (start 4.061 -3.774) (end 4.061 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2c526a69-34c5-46a1-a895-28fb84bea03a))
    (fp_line (start 4.061 1.04) (end 4.061 3.774)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7287e4f5-006e-4f4e-a0a7-2db35cda9bfc))
    (fp_line (start 4.101 -3.757) (end 4.101 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ca607426-a4fb-4f33-b40c-1064e491c872))
    (fp_line (start 4.101 1.04) (end 4.101 3.757)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d4e800c1-4f6f-4ee7-bc2b-eea058d99087))
    (fp_line (start 4.141 -3.74) (end 4.141 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7e3453fa-c732-46c8-bd4f-da81dc3ebe57))
    (fp_line (start 4.141 1.04) (end 4.141 3.74)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 00e60b65-f42e-4b74-8c38-66c48d60cd0e))
    (fp_line (start 4.181 -3.722) (end 4.181 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fe110668-d5ad-4577-b668-82a484c25818))
    (fp_line (start 4.181 1.04) (end 4.181 3.722)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c1d664d0-bc89-4041-b354-e975af132455))
    (fp_line (start 4.221 -3.704) (end 4.221 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9a1930ce-002a-4c98-a27d-ec59113f881b))
    (fp_line (start 4.221 1.04) (end 4.221 3.704)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3e0dbd29-c60e-41f2-b60c-c0f0db99207f))
    (fp_line (start 4.261 -3.686) (end 4.261 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9f24b3ba-4c3b-4d11-a0e6-c38c9dc48b38))
    (fp_line (start 4.261 1.04) (end 4.261 3.686)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e36f5473-26c4-4ca9-87cc-2a88f782e5f6))
    (fp_line (start 4.301 -3.666) (end 4.301 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5e2de1f9-0409-41ef-8b3b-ac41958e8797))
    (fp_line (start 4.301 1.04) (end 4.301 3.666)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7ce40f3f-2dc9-4d0d-be17-212c4342fcd1))
    (fp_line (start 4.341 -3.647) (end 4.341 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 152eb82e-549d-42f0-b9d5-65f5be27e3bf))
    (fp_line (start 4.341 1.04) (end 4.341 3.647)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c7a59b77-56c5-495b-a511-b359061ae688))
    (fp_line (start 4.381 -3.627) (end 4.381 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c3f5a1a9-2ef3-432e-b1eb-992d1f6fad25))
    (fp_line (start 4.381 1.04) (end 4.381 3.627)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2bdec39c-95a0-4484-be26-25fd1551a4ee))
    (fp_line (start 4.421 -3.606) (end 4.421 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1624c689-8449-4a3c-b94b-ce0d70da7d5d))
    (fp_line (start 4.421 1.04) (end 4.421 3.606)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d1f8b9c9-49fd-4483-ba4f-48b532268cb5))
    (fp_line (start 4.461 -3.584) (end 4.461 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f2558eea-a857-481e-a1d9-955813284302))
    (fp_line (start 4.461 1.04) (end 4.461 3.584)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 38b54757-fb38-4a72-8ebf-c742ea9246f2))
    (fp_line (start 4.501 -3.562) (end 4.501 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6f17110d-dbc3-49f4-a884-87ac55e5642f))
    (fp_line (start 4.501 1.04) (end 4.501 3.562)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a89d429c-c31e-4f1b-b966-569164b53295))
    (fp_line (start 4.541 -3.54) (end 4.541 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7c15c2de-6c4a-49c7-88ed-7c3949220774))
    (fp_line (start 4.541 1.04) (end 4.541 3.54)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 878c5517-2b78-446c-b717-cc716cc8d25e))
    (fp_line (start 4.581 -3.517) (end 4.581 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3d023b5c-4dac-41a6-9151-e8e5bbc646be))
    (fp_line (start 4.581 1.04) (end 4.581 3.517)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a72e7eb8-d6e8-4de9-9a75-d89d5023fd25))
    (fp_line (start 4.621 -3.493) (end 4.621 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c4e1590b-2070-421b-886b-0d57963841ad))
    (fp_line (start 4.621 1.04) (end 4.621 3.493)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7fbab591-e419-4a18-bfbb-593bb4b4d4e1))
    (fp_line (start 4.661 -3.469) (end 4.661 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2872a0c7-a857-4de3-814f-4f800a4670bf))
    (fp_line (start 4.661 1.04) (end 4.661 3.469)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 85e5dea0-f44f-46d9-a5cb-f25c1d887e88))
    (fp_line (start 4.701 -3.444) (end 4.701 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1821b551-6918-4204-8df4-2230afe05868))
    (fp_line (start 4.701 1.04) (end 4.701 3.444)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ec1538b6-e45b-4853-a02a-77fbafa388e6))
    (fp_line (start 4.741 -3.418) (end 4.741 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 534e7a57-3184-4a75-b61c-dac57abe26f5))
    (fp_line (start 4.741 1.04) (end 4.741 3.418)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4581d867-f1a4-411e-b6d9-0840cfb8fd37))
    (fp_line (start 4.781 -3.392) (end 4.781 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 68e77061-411b-4c5f-af21-9b94cbd0a4b5))
    (fp_line (start 4.781 1.04) (end 4.781 3.392)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 35fde070-539b-4369-9e8e-3d6b2888783c))
    (fp_line (start 4.821 -3.365) (end 4.821 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c9867d95-3287-4ab8-b7ae-9453dd0e775c))
    (fp_line (start 4.821 1.04) (end 4.821 3.365)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7db00d0a-a73a-4c9a-8195-47e7bdbb5561))
    (fp_line (start 4.861 -3.338) (end 4.861 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f3cfaf32-815b-4ab0-b924-b915192e61ad))
    (fp_line (start 4.861 1.04) (end 4.861 3.338)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 78fcb19f-29ea-4c8f-ba4f-135808c5f02e))
    (fp_line (start 4.901 -3.309) (end 4.901 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 88c56e54-d7a2-4ea3-9926-963ceb1de579))
    (fp_line (start 4.901 1.04) (end 4.901 3.309)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 388c86ab-771a-4053-ba04-02762a7ddbbd))
    (fp_line (start 4.941 -3.28) (end 4.941 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c2b9caf3-7e34-4ddb-80b3-b6775f3397be))
    (fp_line (start 4.941 1.04) (end 4.941 3.28)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0990ef7f-e36f-484e-9096-85d967cd1d37))
    (fp_line (start 4.981 -3.25) (end 4.981 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 086d5972-5cbf-4ed6-b4f5-6673af270bb3))
    (fp_line (start 4.981 1.04) (end 4.981 3.25)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f8703f64-436b-4bed-82d1-c6fafdb6ccbe))
    (fp_line (start 5.021 -3.22) (end 5.021 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 89d8a6ad-9a16-4b57-8b87-753e836542b3))
    (fp_line (start 5.021 1.04) (end 5.021 3.22)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 893095f5-4df3-4bdf-a5b6-bb9666c4c4a5))
    (fp_line (start 5.061 -3.189) (end 5.061 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 392822f0-3320-4b02-9763-35b83ad3e3ba))
    (fp_line (start 5.061 1.04) (end 5.061 3.189)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 034ddb0d-0cf9-4f9b-adab-851674a5a263))
    (fp_line (start 5.101 -3.156) (end 5.101 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a77e0950-2d14-4d2d-b07e-bf7d1ffc4536))
    (fp_line (start 5.101 1.04) (end 5.101 3.156)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e9afafcc-8254-44ec-b5d4-8ecce2965d96))
    (fp_line (start 5.141 -3.124) (end 5.141 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f01c79f1-f12d-40d1-9645-455cfa026dbb))
    (fp_line (start 5.141 1.04) (end 5.141 3.124)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 49874172-19ce-46a7-bcaa-a3a9cc0c1a02))
    (fp_line (start 5.181 -3.09) (end 5.181 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ff9a5a78-cd4b-4830-aa62-ff4da74ff901))
    (fp_line (start 5.181 1.04) (end 5.181 3.09)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4e9a3d9c-0f9c-46bf-9bfa-557f81200403))
    (fp_line (start 5.221 -3.055) (end 5.221 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cba243be-d20b-4e93-a170-cf7060536265))
    (fp_line (start 5.221 1.04) (end 5.221 3.055)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8f654063-5f17-41bf-ab15-f1b784d5350b))
    (fp_line (start 5.261 -3.019) (end 5.261 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e65180f4-5bc2-429c-bef8-512f6215eee9))
    (fp_line (start 5.261 1.04) (end 5.261 3.019)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a224c795-57c1-4e5a-99cf-e4a47ab31522))
    (fp_line (start 5.301 -2.983) (end 5.301 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 624285b7-3140-4060-ad0c-89158866c90c))
    (fp_line (start 5.301 1.04) (end 5.301 2.983)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3ffa2ab3-9ce1-4e4e-8441-fca229cb8c84))
    (fp_line (start 5.341 -2.945) (end 5.341 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e02a58de-8289-441b-a21f-42a899622667))
    (fp_line (start 5.341 1.04) (end 5.341 2.945)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0c6ca5c0-cc57-4b1f-a37c-7a4bde1324a4))
    (fp_line (start 5.381 -2.907) (end 5.381 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0ab85d3f-fefc-475b-b290-c6175f3be945))
    (fp_line (start 5.381 1.04) (end 5.381 2.907)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c077dcf8-f6c9-463b-afd8-5560620f3a84))
    (fp_line (start 5.421 -2.867) (end 5.421 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 40444d41-ba11-410a-acb5-634fb5e1d6a9))
    (fp_line (start 5.421 1.04) (end 5.421 2.867)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 84095926-69ad-4a7c-a3e0-dc571b3df471))
    (fp_line (start 5.461 -2.826) (end 5.461 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0936d33d-4d56-43c7-821e-7b00443a9b34))
    (fp_line (start 5.461 1.04) (end 5.461 2.826)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 011b3b66-167c-4a61-b789-8758ee78cf9e))
    (fp_line (start 5.501 -2.784) (end 5.501 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 55740b58-0f9b-4d29-8dd4-72f34749579c))
    (fp_line (start 5.501 1.04) (end 5.501 2.784)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 043d4c1d-3980-45cd-a10c-bd156c19674c))
    (fp_line (start 5.541 -2.741) (end 5.541 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3df9a525-bb46-440e-8201-30472ab12755))
    (fp_line (start 5.541 1.04) (end 5.541 2.741)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aa629719-6051-485c-ab23-04d8c954a432))
    (fp_line (start 5.581 -2.697) (end 5.581 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 404dc71a-3892-40c5-9623-5b7e00dd89a5))
    (fp_line (start 5.581 1.04) (end 5.581 2.697)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4862764c-7018-4a97-a8f9-bf569234f7b6))
    (fp_line (start 5.621 -2.651) (end 5.621 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c2b2f820-06c3-4427-a80e-7fad0f0f07db))
    (fp_line (start 5.621 1.04) (end 5.621 2.651)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 55256b54-4581-44dc-a792-53cc1ef1f28f))
    (fp_line (start 5.661 -2.604) (end 5.661 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e75cb9a0-4b6f-48d6-91bf-f86a777c8496))
    (fp_line (start 5.661 1.04) (end 5.661 2.604)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 35764d64-0621-4f38-897b-1c360f3527b6))
    (fp_line (start 5.701 -2.556) (end 5.701 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a0cad895-c142-48de-b4f9-a7e5ad448b32))
    (fp_line (start 5.701 1.04) (end 5.701 2.556)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7158294b-d7d5-4ec8-9db1-561a51463ae0))
    (fp_line (start 5.741 -2.505) (end 5.741 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 121d4d17-11ca-45fa-93b2-4d1d515de39a))
    (fp_line (start 5.741 1.04) (end 5.741 2.505)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f0eb4fcf-b687-4254-8018-9d28214b0974))
    (fp_line (start 5.781 -2.454) (end 5.781 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f0a858fa-a486-4eda-8ec4-01343cc21fb2))
    (fp_line (start 5.781 1.04) (end 5.781 2.454)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ef3dca6f-7510-4550-8521-45f04dc59592))
    (fp_line (start 5.821 -2.4) (end 5.821 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cb6c6f3c-4ff0-4a63-adbe-3e04dfaad563))
    (fp_line (start 5.821 1.04) (end 5.821 2.4)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9b36d539-24c6-400e-bd56-983b61f58303))
    (fp_line (start 5.861 -2.345) (end 5.861 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2a0e9500-c6c7-447b-941b-ffd76b5a436b))
    (fp_line (start 5.861 1.04) (end 5.861 2.345)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aa6832e9-37ee-4ddb-bf8c-ca3df884c505))
    (fp_line (start 5.901 -2.287) (end 5.901 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 80c04781-e946-46b8-88e8-108a70c08f14))
    (fp_line (start 5.901 1.04) (end 5.901 2.287)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 23ad37ff-b651-499e-9675-d23c4a00d1bc))
    (fp_line (start 5.941 -2.228) (end 5.941 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c3bdeb29-7c40-425d-bd21-a5f31838e8dc))
    (fp_line (start 5.941 1.04) (end 5.941 2.228)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 124100fd-491f-419b-bcfa-ce8c0ad1fd16))
    (fp_line (start 5.981 -2.166) (end 5.981 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6e18021c-6425-40f7-a976-aa18140d1e62))
    (fp_line (start 5.981 1.04) (end 5.981 2.166)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ea4c79a5-635b-4964-b066-be3954c8c783))
    (fp_line (start 6.021 -2.102) (end 6.021 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4007c6ac-f877-4fd2-a6ee-258a708e1996))
    (fp_line (start 6.021 1.04) (end 6.021 2.102)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6d288162-9a82-48a9-baed-8648496fc94f))
    (fp_line (start 6.061 -2.034) (end 6.061 2.034)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c957040b-d9d3-440f-85b0-784de13b36db))
    (fp_line (start 6.101 -1.964) (end 6.101 1.964)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6468ea20-e863-4424-b7eb-0fe5e9933252))
    (fp_line (start 6.141 -1.89) (end 6.141 1.89)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cbef3b71-11c6-44e1-ac06-f568b2405e63))
    (fp_line (start 6.181 -1.813) (end 6.181 1.813)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 508cbfe7-89b1-4dc8-9cd1-6da883a322eb))
    (fp_line (start 6.221 -1.731) (end 6.221 1.731)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3568a968-28ea-4d83-9415-33589ca95f6d))
    (fp_line (start 6.261 -1.645) (end 6.261 1.645)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dd726222-5663-493e-902a-7445ba4aa695))
    (fp_line (start 6.301 -1.552) (end 6.301 1.552)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7d143a30-249d-4141-b9c7-9e961fd4f379))
    (fp_line (start 6.341 -1.453) (end 6.341 1.453)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2817ce72-f2aa-4a20-9356-63f8db57ad5b))
    (fp_line (start 6.381 -1.346) (end 6.381 1.346)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2eed508e-502b-4941-abec-916f2b2b8436))
    (fp_line (start 6.421 -1.229) (end 6.421 1.229)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 72b42bfd-d3d8-423b-baf9-96e79e1bf7be))
    (fp_line (start 6.461 -1.098) (end 6.461 1.098)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d36d9bcd-a048-40d0-a398-03a0296ed5ef))
    (fp_line (start 6.501 -0.948) (end 6.501 0.948)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7b40a113-e9af-434a-b3f2-52d51a5ab908))
    (fp_line (start 6.541 -0.768) (end 6.541 0.768)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 555feaf5-2c30-4ed6-8216-a208fe1ec1b1))
    (fp_line (start 6.581 -0.533) (end 6.581 0.533)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bfe0c71a-ae96-47e2-b745-d7ca7807f5ad))
    (fp_circle (center 2.5 0) (end 6.62 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp b9199a17-5d6a-4477-83d2-1c8aa2f93264))
    (fp_circle (center 2.5 0) (end 6.75 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 5e0dbb63-457a-4c62-acd4-3ea128dc4beb))
    (fp_line (start -0.926759 -1.7475) (end -0.126759 -1.7475)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 047bdeca-0258-421b-b8d2-0b93fd4b822f))
    (fp_line (start -0.526759 -2.1475) (end -0.526759 -1.3475)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b6f473a5-2752-493f-900c-156ea1b4cad2))
    (fp_circle (center 2.5 0) (end 6.5 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 861e7d27-6fca-4bea-a72c-edcbfff8a5cd))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(U1B-Q)") (pintype "passive") (tstamp bf459f8a-39f4-414b-8245-5fefe02975ac))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "/Output") (pintype "passive") (tstamp f8a4bd2b-1bf4-433b-ba9c-6d02a12c82e3))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D8.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Button_Switch_THT:SW_E-Switch_EG1271_SPDT" (layer "F.Cu")
    (tstamp 34a2169a-301e-4259-a59d-f7ca128db306)
    (at 109 61.8)
    (descr "E-Switch sub miniature slide switch, EG series, SPDT, https://www.e-switch.com/wp-content/uploads/2022/06/EG.pdf")
    (tags "switch SPDT")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Single Pole Single Throw (SPST) switch")
    (property "ki_keywords" "switch lever")
    (path "/ab81cef8-8e55-47b0-9ba6-73dfb33982b5")
    (attr through_hole)
    (fp_text reference "SW1" (at 2.5 -1.65) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp dbc63aec-04b0-426b-8dc9-90a0c3a0fe84)
    )
    (fp_text value "on/off" (at 2.5 5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp bfa61333-7b00-415d-adc4-ba823491857a)
    )
    (fp_text user "${REFERENCE}" (at 2.5 -1.65) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp d232c159-fa73-4d2e-bae4-083f77da7c30)
    )
    (fp_line (start -2.15 -0.55) (end -1.15 -0.55)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 81dd5724-592d-4181-8687-8c3fa62fe32e))
    (fp_line (start -2.15 0.45) (end -2.15 -0.55)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 00b9776b-a9c9-4c78-b748-4653a72dfaef))
    (fp_line (start -1.85 -0.25) (end -1 -0.25)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 66246857-13af-4f69-bd1e-b2c6ca950d9b))
    (fp_line (start -1.85 3.45) (end -1.85 -0.25)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 030fe8a9-f4e0-4abf-b820-c5e751059616))
    (fp_line (start -0.97 3.45) (end -1.85 3.45)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f702581e-e728-4130-aacb-762bc10e4e03))
    (fp_line (start 1 -0.25) (end 1.53 -0.25)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c04375ad-7ba8-467e-a189-4c1fabb87e5b))
    (fp_line (start 1.53 3.45) (end 0.97 3.45)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e7d19dc0-8110-4397-96ad-0e27a29b68c5))
    (fp_line (start 3.47 -0.25) (end 4.03 -0.25)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d351118b-bff4-4272-a1d8-e9ecfdc9bcda))
    (fp_line (start 4.02 3.45) (end 3.47 3.45)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8c004755-183b-4b37-894d-4f2da2f08684))
    (fp_line (start 5.97 -0.25) (end 6.85 -0.25)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e1d70475-0872-4a1b-a18d-b95a816b968b))
    (fp_line (start 6.85 -0.25) (end 6.85 3.45)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ec663bf9-cc7d-4793-9883-8fcd9874ef7f))
    (fp_line (start 6.85 3.45) (end 5.98 3.45)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e9ef48fc-fc21-4fc5-b275-453e114381e3))
    (fp_line (start -2 -1.05) (end 7 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e3ad0ef8-aa4b-4720-9f03-491f6aed3179))
    (fp_line (start -2 4.25) (end -2 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b005cc44-6e9e-4174-b689-966aca568259))
    (fp_line (start 7 -1.05) (end 7 4.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 84ed9816-6d4e-4830-9f76-4c972cfcb763))
    (fp_line (start 7 4.25) (end -2 4.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f0f258b1-977a-4346-84fc-552c24ecd73f))
    (fp_line (start -1.75 -0.15) (end -1.75 3.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3d71e7b0-41bd-4449-8e20-db3560841950))
    (fp_line (start -1.75 -0.15) (end 6.75 -0.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4750ba56-c642-49cb-8a87-beaa65fdaa8a))
    (fp_line (start 0.4 0.6) (end 0.4 2.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 356c790b-1ba7-4fe2-87ec-23ea1ab10ecc))
    (fp_line (start 0.4 0.6) (end 4.6 0.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d87172d3-5d39-44a1-94d2-97e304d8744c))
    (fp_line (start 0.75 0.6) (end 0.75 2.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ea15c57c-1d9c-4496-9205-3761083eb13f))
    (fp_line (start 1.1 0.6) (end 1.1 2.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bdb118a9-cf0b-41d9-a57d-30b810a1fbe0))
    (fp_line (start 1.45 0.6) (end 1.45 2.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c2a9654d-aa7c-433f-baae-14af2f637555))
    (fp_line (start 1.8 0.6) (end 1.8 2.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b01f11c5-21b9-4e15-b231-3ebb985f393d))
    (fp_line (start 2.15 0.6) (end 2.15 2.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 91b7c3ac-1186-4295-8661-e122a651270a))
    (fp_line (start 2.5 0.6) (end 2.5 2.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 658a516a-1f53-4241-8021-84a5b1674ab0))
    (fp_line (start 4.6 0.6) (end 4.6 2.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a85d31ec-0fdf-40ef-8cc8-f7ab65ef3d1c))
    (fp_line (start 4.6 2.6) (end 0.4 2.6)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 26bf514d-387f-4407-ad90-84ebfddbf797))
    (fp_line (start 6.75 -0.15) (end 6.75 3.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9f884fd3-e61c-464a-a340-dde09942b06c))
    (fp_line (start 6.75 3.35) (end -1.75 3.35)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c09c97b9-4743-4947-b914-117e3a9629a9))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(BT1-+)") (pinfunction "A") (pintype "passive") (tstamp 6d552adc-1057-439b-bb49-8e3d1f63c944))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(SW1-B)") (pinfunction "B") (pintype "passive") (tstamp e7916563-0a76-4c59-a004-1dce30473b3a))
    (pad "3" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp f615204c-1cb5-436e-ae17-91e61d12585a))
    (pad "4" thru_hole circle (at 0 3.2) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 43936945-0911-4e9a-94c4-3a22b5781dda))
    (pad "5" thru_hole circle (at 2.5 3.2) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 3344e70e-3b6f-46b4-81f3-c423a67796d9))
    (pad "6" thru_hole circle (at 5 3.2) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask") (tstamp 87437a1b-61db-43ae-94e4-613b7110cd49))
    (model "${KICAD7_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_E-Switch_EG1271_SPDT.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tstamp 3cad26a2-3a51-4727-96c4-16d952b446b2)
    (at 142 113)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7mm width 2.5mm Capacitor")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (path "/cfbbfe94-84c5-45ee-a206-36883b724a0a")
    (attr through_hole)
    (fp_text reference "C1" (at 2.5 -2.5) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7102446d-061a-4355-9a27-5ac1d5f60b79)
    )
    (fp_text value "0.01uF" (at 2.5 2.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 600b4325-b73b-482c-a212-e65c77b77017)
    )
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 480bed18-86a7-4c31-b5d8-a7ea0edf7b2d)
    )
    (fp_line (start -1.12 -1.37) (end -1.12 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 34eab6ba-e94c-426c-9342-022018d88740))
    (fp_line (start -1.12 -1.37) (end 6.12 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 56d79c82-1c79-40e8-8723-faa1812306b7))
    (fp_line (start -1.12 1.37) (end 6.12 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cf47d58b-ac3c-4464-99f5-343f7aa90a31))
    (fp_line (start 6.12 -1.37) (end 6.12 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 48e089e6-fcc0-46c6-8a4a-febe02a4ea14))
    (fp_line (start -1.25 -1.5) (end -1.25 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 09619e61-6f2d-4730-a376-e314b6af5f7e))
    (fp_line (start -1.25 1.5) (end 6.25 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp d5ba7bf9-818d-43ad-ae32-9d72a62087b9))
    (fp_line (start 6.25 -1.5) (end -1.25 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8cdb4898-ff0a-40fe-b37f-8a928715d04c))
    (fp_line (start 6.25 1.5) (end 6.25 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 70a8fa67-2f01-4396-950e-cbe8d0c35929))
    (fp_line (start -1 -1.25) (end -1 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 60c62af0-9be9-4f19-8f5a-899b54a34204))
    (fp_line (start -1 1.25) (end 6 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 829ff214-f462-4033-a7c9-b33ec52fe3b3))
    (fp_line (start 6 -1.25) (end -1 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 19825342-57af-46f2-810d-d506c7c5880f))
    (fp_line (start 6 1.25) (end 6 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 834337c8-5c4f-4bc1-be75-d056617acb32))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U1A-THR)") (pintype "passive") (tstamp 567e2e44-39db-447a-b53f-25c783504edb))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(BT1--)") (pintype "passive") (tstamp 0d1e1d5f-ecf7-4375-9521-46eca813a236))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tstamp 4d83923d-9040-4196-84f9-6740e2fff802)
    (at 98.4075 62.32 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Multiple-cell battery")
    (property "ki_keywords" "batt voltage-source cell")
    (path "/1b5c3dca-c959-4afa-8708-51a0fbbc37cc")
    (attr through_hole)
    (fp_text reference "BT1" (at 2.54 -5.08 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 85fd92e4-899e-473b-b829-b7770d00c943)
    )
    (fp_text value "9V" (at 2.54 5.08 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 919dbf68-2b0a-4098-9907-adafa38ca6ec)
    )
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 046a9152-3e07-4b50-a5d7-5ca267af82db)
    )
    (fp_line (start -2.54 -3.81) (end -2.54 3.81)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dd175232-670f-4492-a2a1-5478d09bcc86))
    (fp_line (start -2.54 3.81) (end 7.62 3.81)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e9203835-8f5b-4b33-96f3-148e0fad7efc))
    (fp_line (start 7.62 -3.81) (end -2.54 -3.81)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cab11a95-0206-43f2-8ca7-73537e67edf1))
    (fp_line (start 7.62 2.54) (end -2.54 2.54)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5a1ace32-e41d-493b-b70d-581a0616c5eb))
    (fp_line (start 7.62 3.81) (end 7.62 -3.81)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8a9b58af-91db-4d61-8eac-7ef2b020959e))
    (fp_line (start -2.71 -4) (end -2.71 4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 58453901-3e03-4061-9383-683c38fb2dc0))
    (fp_line (start -2.71 -4) (end 7.79 -4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b442b483-fe0f-4aff-9982-43917a3e36fd))
    (fp_line (start 7.79 4) (end -2.71 4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9a41caa2-1ee1-4f6f-bf7e-b85860148f75))
    (fp_line (start 7.79 4) (end 7.79 -4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b4216861-ff20-4787-afd1-225034dfb349))
    (fp_line (start -2.46 -3.75) (end -2.46 3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5ed35661-b9e8-49d4-b276-7c18014e0b12))
    (fp_line (start -2.46 3.75) (end 7.54 3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6a529d38-56aa-41d0-a8a9-5eaa49d75933))
    (fp_line (start -2.41 2.55) (end 7.49 2.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7aa9343c-7964-4116-8f79-d0acedee3cc9))
    (fp_line (start 7.54 -3.75) (end -2.46 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 79870bfa-5322-498f-b7c4-5dcd32ecde60))
    (fp_line (start 7.54 3.75) (end 7.54 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f3ce8ad2-f29d-4028-bc6e-d2519e2cb610))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(BT1-+)") (pinfunction "+") (pintype "passive") (tstamp 3f3c01bb-dd05-4dce-8b1d-8a16bf1c213c))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(BT1--)") (pinfunction "-") (pintype "passive") (tstamp e746b775-ae84-4209-9f07-b8e6a9bde973))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tstamp 624c2c30-583e-467d-833a-ef30976fa7fc)
    (at 158 73.19 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/49ca9de9-6005-40f6-9ce0-ed53d08102a2")
    (attr through_hole)
    (fp_text reference "R4" (at 3.81 -1.92 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 56bac40a-50f6-49f9-9052-53765b8271f4)
    )
    (fp_text value "330" (at 3.81 1.92 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a6638302-82e8-40f7-bf96-58289d36f9a4)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab")
        (effects (font (size 0.72 0.72) (thickness 0.108)))
      (tstamp 7d06ac8d-1f9d-4ee1-87cb-27b978fa1e79)
    )
    (fp_line (start 0.94 0) (end 1.89 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e81df98c-a5ef-4084-871d-be916edae4d8))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b12eff63-7046-41f9-b6bc-ce2130552c24))
    (fp_line (start 1.89 0.92) (end 5.73 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3d39bbf3-71d8-4efd-a816-83843c5d22f2))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d8e730fc-1089-485b-b2e9-eb4445fb5653))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 856e64dd-78a1-47f9-b4a3-993d5b673586))
    (fp_line (start 6.68 0) (end 5.73 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 676c1617-458b-4f85-b011-e6429efaadaa))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 39b9f7f3-2c19-4088-bc4a-25fe28327fb2))
    (fp_line (start -0.95 1.05) (end 8.57 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 68d531f8-846a-4fe4-a543-2d1860877bf5))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8e53dbbc-6d51-4fa6-b4e5-dfec732632e6))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 306e8ea2-ff90-4e84-9ff5-5171bac6bf59))
    (fp_line (start 0 0) (end 2.01 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cd883e0d-54d6-4ad5-8db8-5318e2dab026))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8d7fc1b2-0577-4d41-b90b-e7eb9ef3c456))
    (fp_line (start 2.01 0.8) (end 5.61 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 76446b4e-2ee1-4626-91b3-390f07e35e05))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9abe3711-c5a2-4632-bb5c-a9299b05c877))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c76d81ac-c2ba-4956-960a-24e1d17c3d00))
    (fp_line (start 7.62 0) (end 5.61 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 74b7ab0e-45fa-4547-8e84-3f69b81dab74))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(R4-Pad1)") (pintype "passive") (tstamp f253f837-c6da-4614-9179-21be74fb0e10))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(U1B-DIS)") (pintype "passive") (tstamp 8eb55637-a7c4-4b64-a5e9-f6d57bd02ddf))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tstamp 95696f21-095d-4a03-8657-ee55018997ff)
    (at 117 70.38 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/f2e0a5d2-66b4-4e3f-a738-f6b8da1a558e")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 -1.92 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fd560db1-0a68-489e-af59-6c21d8b870d4)
    )
    (fp_text value "470" (at 3.81 1.92 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2d6be13f-e1a6-4a3e-8e53-85f56429eb06)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab")
        (effects (font (size 0.72 0.72) (thickness 0.108)))
      (tstamp 8db6a4a8-a8e6-4e05-bbc4-ad5c7022e546)
    )
    (fp_line (start 0.94 0) (end 1.89 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e909668c-2bc2-4aa0-9b47-765b1a5d413b))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4bd0bd11-965d-4a82-b83f-8721c451f116))
    (fp_line (start 1.89 0.92) (end 5.73 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 71908a50-0b76-41c4-8f94-1bc49305cbb4))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 887942be-e0e4-4de3-aea7-56123ab2a1df))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5c7e43d4-ace4-46c6-8bbd-9e8a952847c1))
    (fp_line (start 6.68 0) (end 5.73 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 447629e9-bd28-4e3d-b274-bb3b5a10a12f))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 92a62666-8cc1-40fa-96a6-9a22c9d0abc9))
    (fp_line (start -0.95 1.05) (end 8.57 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e7897cf2-8311-4749-aa79-7abff9fb5ecc))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8f8edde6-72b4-4eb9-a277-161972d8bc32))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cd680e20-7d04-47b1-a665-d13393b17c00))
    (fp_line (start 0 0) (end 2.01 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp beb62992-2d7c-465a-a9c2-327fdf031045))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 456a4cd1-a402-4027-852c-8d69c9ec3323))
    (fp_line (start 2.01 0.8) (end 5.61 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 38a5388e-93f8-4b44-9c21-a913c57d1b26))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 397d2a54-e97c-4419-bd5c-ef27825ba44d))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 945ee493-8021-4c32-b41b-6aa9d55a571b))
    (fp_line (start 7.62 0) (end 5.61 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3fc849bb-01f9-4616-84e8-e867e1fde85a))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(SW1-B)") (pintype "passive") (tstamp b1abe1c3-e43f-40dd-b2d0-31cc4433d4ae))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D1-A)") (pintype "passive") (tstamp 84aa42f2-7984-4390-b7bc-9ae38df9fbb7))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:C_Disc_D7.0mm_W2.5mm_P5.00mm" (layer "F.Cu")
    (tstamp aaff2537-744b-4e32-84a0-9a366b0d5d5b)
    (at 168.5 106)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=7*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 7mm width 2.5mm Capacitor")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (path "/21739dd9-1439-47ad-b473-9c36483d8152")
    (attr through_hole)
    (fp_text reference "C2" (at 2.5 -2.5) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cad0d0c2-794d-4ed5-bb60-eafd8e6ff8de)
    )
    (fp_text value "0.1uF" (at 2.5 2.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c20e3f03-4905-4af3-a7ae-25ec33ec8324)
    )
    (fp_text user "${REFERENCE}" (at 2.24 0) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c59b334f-0a8e-4acd-aeff-98a4e7dc1e14)
    )
    (fp_line (start -1.12 -1.37) (end -1.12 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a4db8d76-3511-4ca8-bed6-a41eb60015b0))
    (fp_line (start -1.12 -1.37) (end 6.12 -1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f3841b8c-2ec1-4174-b342-9f664ed2fed3))
    (fp_line (start -1.12 1.37) (end 6.12 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 24873a7c-cfe1-489f-83b4-74e8b93bd938))
    (fp_line (start 6.12 -1.37) (end 6.12 1.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4a56dd90-cb00-485f-ba1b-9e97a37c14dc))
    (fp_line (start -1.25 -1.5) (end -1.25 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6e76ec16-24c6-4a54-a15d-f742d946a259))
    (fp_line (start -1.25 1.5) (end 6.25 1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fc9b75f6-897e-46d2-9d8f-94e568088dca))
    (fp_line (start 6.25 -1.5) (end -1.25 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3f51fe53-e446-4f5f-99d8-b3e9dd923215))
    (fp_line (start 6.25 1.5) (end 6.25 -1.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e989d737-569e-43da-8494-6b835eefc768))
    (fp_line (start -1 -1.25) (end -1 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1530ba0b-6661-48ba-b6bd-e9746279d13f))
    (fp_line (start -1 1.25) (end 6 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d99ab4ae-45e6-42f2-83d4-44632e296f27))
    (fp_line (start 6 -1.25) (end -1 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 820e54a6-6a7c-421b-9987-eea2db78892f))
    (fp_line (start 6 1.25) (end 6 -1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8925abc9-844f-46c4-9e0f-fd0e617bd582))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(U1B-DIS)") (pintype "passive") (tstamp 0784d7da-cfb1-4564-b63d-27076d30a1f3))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(BT1--)") (pintype "passive") (tstamp fe65c9b2-d771-4ca7-8990-0a1d8a7a0436))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D7.0mm_W2.5mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-14_W7.62mm_Socket" (layer "F.Cu")
    (tstamp b3000ac7-5ca9-4db4-b3f2-721cd1d1808c)
    (at 140.31 78.7)
    (descr "14-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Dual Timer, DIP-14/SOIC-14")
    (property "ki_keywords" "dual timer")
    (path "/ec864112-fa6e-4828-a076-23e82e2d7f55")
    (attr through_hole)
    (fp_text reference "U1" (at 3.81 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1e01407a-04e5-4b8b-abb4-c4c9a7451503)
    )
    (fp_text value "LM556" (at 3.81 17.57) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2cda5bc5-fc7b-4d63-b65f-92e356a8b062)
    )
    (fp_text user "${REFERENCE}" (at 3.81 7.62) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2380bcfd-6911-4662-a49c-61bac126d3c3)
    )
    (fp_line (start -1.33 -1.39) (end -1.33 16.63)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 09fd8790-2ffc-4c01-891b-d678b538358b))
    (fp_line (start -1.33 16.63) (end 8.95 16.63)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f0a90ad6-5e92-401c-bdf8-e81076a62501))
    (fp_line (start 1.16 -1.33) (end 1.16 16.57)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b4dc149b-aa7b-416b-a6cc-484fb1de41c5))
    (fp_line (start 1.16 16.57) (end 6.46 16.57)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f0b881a5-6445-4e56-ae48-b7e75c013fa0))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c2fe2cff-edf8-4915-9976-403ad4d853b4))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 60bf4721-d89e-40bd-8f75-5e99e1436a47))
    (fp_line (start 6.46 16.57) (end 6.46 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ac4fce7b-14de-41d0-b19f-dc9a63c1581c))
    (fp_line (start 8.95 -1.39) (end -1.33 -1.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e55df364-0466-4760-b271-47fc7a128fcc))
    (fp_line (start 8.95 16.63) (end 8.95 -1.39)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dd631a2e-3ca9-471f-93bd-bd19eb861444))
    (fp_arc (start 4.81 -1.33) (mid 3.81 -0.33) (end 2.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 232e9e16-2f50-4f3a-8ae9-0664dfea780c))
    (fp_line (start -1.55 -1.6) (end -1.55 16.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0eb483bd-e1ae-495f-a28d-23208fdb5d85))
    (fp_line (start -1.55 16.85) (end 9.15 16.85)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 14b9434f-16b4-4873-84d0-0fafe8955485))
    (fp_line (start 9.15 -1.6) (end -1.55 -1.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 40a6a497-0dbb-4e15-9cc5-a7ce742f0c01))
    (fp_line (start 9.15 16.85) (end 9.15 -1.6)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8c2dc4c1-f398-48d8-addd-5211131cdd05))
    (fp_line (start -1.27 -1.33) (end -1.27 16.57)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 577478a6-74ea-42a3-84df-44d3aa06de38))
    (fp_line (start -1.27 16.57) (end 8.89 16.57)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7ab249bd-b810-4e2a-b7b2-0f132cbf7165))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9571acbf-b172-43c1-9c4b-0a73c6b38255))
    (fp_line (start 0.635 16.51) (end 0.635 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 17cc4e13-1891-4397-83d5-cdbebf0b593e))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e05a0c34-0e76-4c2e-8eaa-afb43a314f62))
    (fp_line (start 6.985 -1.27) (end 6.985 16.51)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 775166a7-19e0-4993-b4d5-e5505c92fe02))
    (fp_line (start 6.985 16.51) (end 0.635 16.51)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 68df9bf8-2bf0-41b2-935e-3c5d252c0258))
    (fp_line (start 8.89 -1.33) (end -1.27 -1.33)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9afb7297-49be-44d2-ba53-f070b2a3c63c))
    (fp_line (start 8.89 16.57) (end 8.89 -1.33)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6061e6fb-0394-4dd9-9dca-6053d5686b46))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1A-DIS)") (pinfunction "DIS") (pintype "input") (tstamp 48afc4a8-673f-4c3d-9069-1d3aac4d0128))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U1A-THR)") (pinfunction "THR") (pintype "input") (tstamp 4f910f2e-2e9d-431a-91b7-b59690d5614d))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(U1A-CV-Pad3)") (pinfunction "CV") (pintype "input") (tstamp 1f72c6d6-2f5a-4cbe-a466-bbd001900e43))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(SW1-B)") (pinfunction "R") (pintype "input") (tstamp 2a6fce27-cf9e-4aa4-b1bd-9afc5411baca))
    (pad "5" thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(U1A-Q)") (pinfunction "Q") (pintype "output") (tstamp 6cd40fad-cd5d-4151-9147-e4c0de60e8bf))
    (pad "6" thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U1A-THR)") (pinfunction "TR") (pintype "input") (tstamp 6c8a8775-fa76-4136-a918-3418cc4d0091))
    (pad "7" thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(BT1--)") (pinfunction "GND") (pintype "power_in") (tstamp 2d601240-845b-403d-a74a-7e2511d2b0ab))
    (pad "8" thru_hole oval (at 7.62 15.24) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(U1A-Q)") (pinfunction "TR") (pintype "input") (tstamp 3a828b04-e997-441c-a164-c8b33d6f5272))
    (pad "9" thru_hole oval (at 7.62 12.7) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(U1B-Q)") (pinfunction "Q") (pintype "output") (tstamp 5c41fffa-05a1-4d31-9c57-892c34d713a2))
    (pad "10" thru_hole oval (at 7.62 10.16) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(SW1-B)") (pinfunction "R") (pintype "input") (tstamp ee51d768-8ed6-4489-a587-54ecae7bf71e))
    (pad "11" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "unconnected-(U1B-CV-Pad11)") (pinfunction "CV") (pintype "input") (tstamp 6bfe692c-0df7-4249-bed9-2c7f8226ac45))
    (pad "12" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(U1B-DIS)") (pinfunction "THR") (pintype "input") (tstamp 6bcceb7d-20b0-40a8-b908-4baafc46317f))
    (pad "13" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(U1B-DIS)") (pinfunction "DIS") (pintype "input") (tstamp 9304ba86-1472-4ad8-ab21-aafd06d1d6b4))
    (pad "14" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(SW1-B)") (pinfunction "VCC") (pintype "power_in") (tstamp 78b21426-60cc-4738-ac1f-a22cc68cc39f))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-14_W7.62mm_Socket.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Potentiometer_THT:Potentiometer_Alps_RK09K_Single_Vertical" (layer "F.Cu")
    (tstamp bef89459-16e9-4717-b573-40dc0eacf120)
    (at 145.5 67.05 90)
    (descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
    (tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (path "/d188b2be-a5b2-4f12-a252-322feb4352d9")
    (attr through_hole)
    (fp_text reference "RV2" (at 6.05 -5.15 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 999d36e6-a7a3-4b8d-b1f3-febcb1c56179)
    )
    (fp_text value "470K" (at 6.05 10.15 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 32d0e3b5-afb3-4a14-8d7c-b05a1b658ad9)
    )
    (fp_text user "${REFERENCE}" (at 2 2.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b2456cd0-b2fc-4eec-8cc2-f5761c7770af)
    )
    (fp_line (start 0.88 -2.521) (end 0.88 -1.2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b671bfb2-fde8-42a8-83ac-8f87c8f3510c))
    (fp_line (start 0.88 -2.521) (end 4.817 -2.521)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c1c032c1-8988-46da-be3b-489600bfe8e1))
    (fp_line (start 0.88 1.25) (end 0.88 1.63)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a43e46c6-02e6-4399-b65f-3b0e51c9b9c2))
    (fp_line (start 0.88 3.371) (end 0.88 4.13)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aad79ccb-c46c-4987-a847-93234d91d6e4))
    (fp_line (start 0.88 5.87) (end 0.88 7.52)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2eeb5c0b-12f8-4836-8942-970b7ec916d6))
    (fp_line (start 0.88 7.52) (end 4.817 7.52)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f8ea8310-3248-4c8b-8362-825f94aef928))
    (fp_line (start 9.184 -2.521) (end 13.12 -2.521)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dc3a37af-e665-4ee5-ba1c-aff21dd94d99))
    (fp_line (start 9.184 7.52) (end 13.12 7.52)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 120877b0-3ff5-43d1-a5e1-7eba20bc7181))
    (fp_line (start 13.12 -2.521) (end 13.12 7.52)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9176ad1e-cd63-4cb2-8a00-26094e7abb95))
    (fp_line (start -1.15 -4.15) (end -1.15 9.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 451d61e0-00fa-4d35-bbba-2c87c2db9e27))
    (fp_line (start -1.15 9.15) (end 13.25 9.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6e747d78-140d-48e2-b669-915ae4bd5acc))
    (fp_line (start 13.25 -4.15) (end -1.15 -4.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 05ad338f-7021-4600-ab34-030734d74b26))
    (fp_line (start 13.25 9.15) (end 13.25 -4.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 603a5347-d1df-48fb-aaf8-8021c8050f88))
    (fp_line (start 1 -2.4) (end 1 7.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 41e9349d-b4df-45b7-9675-d7d8b5e194cb))
    (fp_line (start 1 7.4) (end 13 7.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 46a0f5cc-b1c4-4f8a-a5fb-0645bdd53b57))
    (fp_line (start 13 -2.4) (end 1 -2.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dc000b8d-02ba-438e-b199-a4c46c2b0a95))
    (fp_line (start 13 7.4) (end 13 -2.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ce375a78-5556-41d5-b558-507ceaf357e7))
    (fp_circle (center 7.5 2.5) (end 10.5 2.5)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 5e9fb509-ddd7-4ca7-be6a-a9d3c8e9f615))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(SW1-B)") (pinfunction "1") (pintype "passive") (tstamp e1d490f8-5a5d-43df-85fd-d3fb8d6e9a94))
    (pad "2" thru_hole circle (at 0 2.5 90) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(SW1-B)") (pinfunction "2") (pintype "passive") (tstamp 4a4b795b-09d3-4600-835d-0238e2075664))
    (pad "3" thru_hole circle (at 0 5 90) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(R4-Pad1)") (pinfunction "3") (pintype "passive") (tstamp 2c4539d7-3e3b-4576-a397-ca359835ce7e))
    (pad "MP" thru_hole roundrect (at 7 -1.9 90) (size 4 3) (drill oval 2.1 1.8) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp c8567a00-3fc3-45c6-b254-bef235ae0978))
    (pad "MP" thru_hole roundrect (at 7 6.9 90) (size 4 3) (drill oval 2.1 1.8) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 096e243a-998e-4762-b7ad-be2dfaa46a45))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tstamp c38b606d-c266-493c-9a64-7d3593e67669)
    (at 132 97.81 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/e6a40030-3176-4728-b431-e0dd566b4832")
    (attr through_hole)
    (fp_text reference "R2" (at 3.81 -1.92 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 1514de77-194f-41e2-8fef-a9b2c8f6b443)
    )
    (fp_text value "1K" (at 3.81 1.92 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c050f9a1-c3d8-4d77-aa58-ab3e0cd423c8)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab")
        (effects (font (size 0.72 0.72) (thickness 0.108)))
      (tstamp 5378de05-f3f6-4f31-ac8f-52373fb1df3c)
    )
    (fp_line (start 0.94 0) (end 1.89 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d9855a1d-6ba6-47d0-9eab-156985cdddef))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a7eefa4b-54dd-478a-acf6-5196792cd318))
    (fp_line (start 1.89 0.92) (end 5.73 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8b14e854-1410-4b51-b3e3-7ee82e51401a))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f1163056-9bd0-4063-95dd-ed32c3844254))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 673e2240-75ee-4a40-ac76-0f6df960f34f))
    (fp_line (start 6.68 0) (end 5.73 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cb5f74e8-fa0c-47b3-a7ca-39b63ff47c23))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 86f72cad-eb44-4dc4-9ac2-e00813263891))
    (fp_line (start -0.95 1.05) (end 8.57 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 3fb1dc09-7960-4bdd-b36d-32937f5a0b13))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b3209cc2-a9c5-4c3a-81e2-f95ba796dde9))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f742a836-6977-4f3e-99d8-d309ca7556e6))
    (fp_line (start 0 0) (end 2.01 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0d9e027a-f26e-4dfa-840d-224990c0daa4))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4c4db56a-7fed-4c75-9ee4-0c7090eff011))
    (fp_line (start 2.01 0.8) (end 5.61 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dc972aa8-3ed5-42c4-81b2-76d2fff4f23b))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2293f798-8fd3-4848-97a3-3ee1ffb8cbde))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 90dda761-cd92-497e-9d62-5ecbc5d7cf75))
    (fp_line (start 7.62 0) (end 5.61 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e6e23dd5-c8a8-42ef-bd33-e43d9cfe79c9))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(U1A-THR)") (pintype "passive") (tstamp 46981269-50b5-483b-aa53-da0691509ebb))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1A-DIS)") (pintype "passive") (tstamp b4ca85e1-bbb9-4198-8814-7cde7ef9c6a8))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tstamp c6a9692b-f046-437d-a2de-a6f675092e64)
    (at 125.19 83)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/7394ddd4-ced1-40e4-bce1-8d6e48c05250")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 -1.92) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 3e51d1c2-e31b-4e15-b556-fff2c0b0604a)
    )
    (fp_text value "330" (at 3.81 1.92) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 795644ab-2d9b-4798-a124-d9b77919bd11)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab")
        (effects (font (size 0.72 0.72) (thickness 0.108)))
      (tstamp 7173cb6e-c2fc-4334-9e2c-8a14137b7ed5)
    )
    (fp_line (start 0.94 0) (end 1.89 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e15dbd7c-7fdc-481b-9f36-4db9c18df6cb))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 52f1916e-867a-428b-b73a-712794bad305))
    (fp_line (start 1.89 0.92) (end 5.73 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d6bf8b68-5e70-490a-a168-bcdfc8891caf))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d9829be1-5a65-4990-a702-e32b93b44c2b))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 977332ed-eb59-4d9a-8322-80564cf34540))
    (fp_line (start 6.68 0) (end 5.73 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7fd227df-9cbc-4e1f-b84a-2573f9228b43))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 545e9897-4a4e-4b42-8f19-9753466336b6))
    (fp_line (start -0.95 1.05) (end 8.57 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5c82162c-d1e8-466b-bc47-d366b2a87e22))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f192db4d-0a3a-41a3-862b-f57c4db37bdc))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 01b39b18-708e-4f02-9df5-8cb83022dcbe))
    (fp_line (start 0 0) (end 2.01 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1c742f1d-49bd-4d60-ba5e-5242d71f2a64))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ffd6a08d-b7be-4645-ab7d-7459887f5282))
    (fp_line (start 2.01 0.8) (end 5.61 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ace9b7fb-0671-4d60-9c1d-7963f58ba91b))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 368f54b5-25ea-46c5-a18f-2b066231e4c0))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 539535d7-f385-4110-962e-4c20d88d876a))
    (fp_line (start 7.62 0) (end 5.61 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4b4ec8b7-dd1d-4d23-960a-804fc975d19d))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(R3-Pad1)") (pintype "passive") (tstamp 8eb2c676-8d70-4624-ab8e-f9dc840e079e))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1A-DIS)") (pintype "passive") (tstamp 78ac036b-c256-43a3-b609-87cc7dd0bf95))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TerminalBlock:TerminalBlock_bornier-2_P5.08mm" (layer "F.Cu")
    (tstamp d5d74439-dc88-41f5-a0b0-43c493786e09)
    (at 187 83 -90)
    (descr "simple 2-pin terminal block, pitch 5.08mm, revamped version of bornier2")
    (tags "terminal block bornier2")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Speaker")
    (property "ki_keywords" "speaker sound")
    (path "/8c779346-06ef-40ed-b00f-403be39d2895")
    (attr through_hole)
    (fp_text reference "LS1" (at 2.54 -5.08 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 60cffbcf-7d31-4792-98a0-1d957d6cc080)
    )
    (fp_text value "Speaker" (at 2.54 5.08 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 54e912d5-85c5-40a1-89b4-7bd936760cfc)
    )
    (fp_text user "${REFERENCE}" (at 2.54 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6e7756c5-3ae4-4e8e-bc8e-7dbf904524c0)
    )
    (fp_line (start -2.54 -3.81) (end -2.54 3.81)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp da4007ed-74cf-4c80-a04a-1aacc5576ee3))
    (fp_line (start -2.54 3.81) (end 7.62 3.81)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bb1cfbb0-0c60-48a2-8667-fef797e2d7c2))
    (fp_line (start 7.62 -3.81) (end -2.54 -3.81)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9fa6d50d-1d63-4d18-a119-e1b2c35e896a))
    (fp_line (start 7.62 2.54) (end -2.54 2.54)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 77ef6221-bece-4285-b74a-f86c59d74627))
    (fp_line (start 7.62 3.81) (end 7.62 -3.81)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp be220a55-4c48-4afc-a4f6-ff3355651284))
    (fp_line (start -2.71 -4) (end -2.71 4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 256fe8e2-9c83-48b9-96d3-00f2d9ccea95))
    (fp_line (start -2.71 -4) (end 7.79 -4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 42ecff9a-92cd-4a90-972a-fe75b0704ffc))
    (fp_line (start 7.79 4) (end -2.71 4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 31367cc2-321d-499b-8407-72bd5ae8dbfa))
    (fp_line (start 7.79 4) (end 7.79 -4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fcfe3711-6b0c-4935-8d20-85945e2177ea))
    (fp_line (start -2.46 -3.75) (end -2.46 3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6056a7d8-9a70-4eeb-adf8-0bc30634e85d))
    (fp_line (start -2.46 3.75) (end 7.54 3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 307f3010-f627-4179-becd-b13a8bb27bb6))
    (fp_line (start -2.41 2.55) (end 7.49 2.55)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4a9c7910-012b-4e84-9bb3-09fabce1e043))
    (fp_line (start 7.54 -3.75) (end -2.46 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5fee5c51-3d68-4994-be29-5fba988fed1d))
    (fp_line (start 7.54 3.75) (end 7.54 -3.75)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3f7c4976-9a0d-4239-a18a-113f47ff8559))
    (pad "1" thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 6 "/Output") (pinfunction "1") (pintype "input") (tstamp 4a7a74b6-ee80-4f24-b0ef-1223e9c33b80))
    (pad "2" thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(BT1--)") (pinfunction "2") (pintype "input") (tstamp befe91e1-2e30-41ed-a678-d86a6c90fd4d))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_bornier-2_P5.08mm.wrl"
      (offset (xyz 2.539999962 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Potentiometer_THT:Potentiometer_Alps_RK09K_Single_Vertical" (layer "F.Cu")
    (tstamp e216eda1-8e43-4124-bcfd-5095b6262643)
    (at 126 67 90)
    (descr "113004U 1130A6S 11300DR 1130A8G 1130081 1130A5R 1130AP5 1130AST  D1130C3W D1130C1B D1130C3C D1130C2P Potentiometer, vertical, Alps RK09K Single, https://tech.alpsalpine.com/prod/e/pdf/potentiometer/rotarypotentiometers/rk09k/rk09k.pdf")
    (tags "Potentiometer vertical Alps RK09K RK09D Single Snapin")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (path "/77856a4f-e213-4b7d-80b8-6ae03b0c3fc6")
    (attr through_hole)
    (fp_text reference "RV1" (at 6.05 -5.15 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8f82c77d-6f39-4088-a85e-fcb60469f704)
    )
    (fp_text value "470K" (at 6.05 10.15 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 0bf27dc3-d27e-45be-a476-27080ca23f46)
    )
    (fp_text user "${REFERENCE}" (at 2 2.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fe320a4c-c11c-4035-9b55-d2221ef744cb)
    )
    (fp_line (start 0.88 -2.521) (end 0.88 -1.2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a213869c-ccee-4c67-8b65-1d5b13247e77))
    (fp_line (start 0.88 -2.521) (end 4.817 -2.521)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6dc0127d-f1ff-4ad0-9089-68a690d9a596))
    (fp_line (start 0.88 1.25) (end 0.88 1.63)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 22673c2b-72f2-4de8-94c9-6fb77b9aeb4d))
    (fp_line (start 0.88 3.371) (end 0.88 4.13)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e0c8b400-16cc-4f5b-8319-3313e05472bd))
    (fp_line (start 0.88 5.87) (end 0.88 7.52)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 464b8a0f-fe8a-4996-ac50-f9d9cf596a4a))
    (fp_line (start 0.88 7.52) (end 4.817 7.52)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bb8ea7b6-f1e2-4956-aec7-378cec982c05))
    (fp_line (start 9.184 -2.521) (end 13.12 -2.521)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9f62e0cf-0838-418a-9877-7d48ddcaae35))
    (fp_line (start 9.184 7.52) (end 13.12 7.52)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2823a134-3d0b-4407-b99d-91e176ef9d95))
    (fp_line (start 13.12 -2.521) (end 13.12 7.52)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d2d9cbb1-dcf7-4117-a68b-3f1bffb29e5a))
    (fp_line (start -1.15 -4.15) (end -1.15 9.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 01d37708-481e-4473-bfa5-0003d039ddc6))
    (fp_line (start -1.15 9.15) (end 13.25 9.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c66f9f7e-dc09-4e24-8f38-f3ed5b8f1542))
    (fp_line (start 13.25 -4.15) (end -1.15 -4.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp c1e2a1e3-3669-4d42-ae1b-bc97f3321092))
    (fp_line (start 13.25 9.15) (end 13.25 -4.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 49fd80f3-95ff-4388-b06b-b57ff9c1d8c4))
    (fp_line (start 1 -2.4) (end 1 7.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 88c0bd39-63b3-424a-b809-88d21612c948))
    (fp_line (start 1 7.4) (end 13 7.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3e200b4c-1cc9-4622-8429-6376fd579132))
    (fp_line (start 13 -2.4) (end 1 -2.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5a7227f7-3db1-458e-97e0-8cece492c1e4))
    (fp_line (start 13 7.4) (end 13 -2.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp faed255e-0c79-458a-8a4c-02d703810645))
    (fp_circle (center 7.5 2.5) (end 10.5 2.5)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 2b509f06-533b-4a2b-a2d6-da7b48c077c1))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(SW1-B)") (pinfunction "1") (pintype "passive") (tstamp 851bd435-b152-42c1-ad90-d4f457bbe513))
    (pad "2" thru_hole circle (at 0 2.5 90) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(SW1-B)") (pinfunction "2") (pintype "passive") (tstamp 984147e7-cbd4-44de-aa35-8f052ec57fcd))
    (pad "3" thru_hole circle (at 0 5 90) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(R3-Pad1)") (pinfunction "3") (pintype "passive") (tstamp c320d205-ac48-4506-820d-bd208199900c))
    (pad "MP" thru_hole roundrect (at 7 -1.9 90) (size 4 3) (drill oval 2.1 1.8) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp edc38f3c-1d06-439b-ac4a-2a499dd01e0b))
    (pad "MP" thru_hole roundrect (at 7 6.9 90) (size 4 3) (drill oval 2.1 1.8) (layers "*.Cu" "*.Mask") (roundrect_rratio 0.25) (tstamp 520dc4a5-6230-43ea-8d2b-315dd42db454))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Alps_RK09K_Single_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "LED_THT:LED_D5.0mm" (layer "F.Cu")
    (tstamp f48ed147-9ce5-4fde-a5fe-ed2821edf762)
    (at 108.46 73)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "atari_punk_console.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (path "/2614fffd-3a54-467d-8220-f5af5ce4887d")
    (attr through_hole)
    (fp_text reference "D1" (at 1.27 -3.96) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f674147f-47d7-4b67-a537-4c76952a395a)
    )
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 7091b62b-2648-4ba6-9276-75c1ce83a072)
    )
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab")
        (effects (font (size 0.8 0.8) (thickness 0.2)))
      (tstamp 386b9e6c-942c-449d-8b66-fb4356df8468)
    )
    (fp_line (start -1.29 -1.545) (end -1.29 1.545)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e9ad5214-03db-4138-b993-d04c3aa794f0))
    (fp_arc (start -1.29 -1.54483) (mid 2.072002 -2.880433) (end 4.26 0.000462)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 04ba16f0-9b9c-44e8-a0e4-941c043fde86))
    (fp_arc (start 4.26 -0.000462) (mid 2.072002 2.880433) (end -1.29 1.54483)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d9b65dfa-aa46-4f75-baee-bbd0b6784645))
    (fp_circle (center 1.27 0) (end 3.77 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 8b551056-e13f-477c-9274-ed84c36d4a78))
    (fp_line (start -1.95 -3.25) (end -1.95 3.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e9bd3c16-aa38-471a-b6a4-dd1ecad60907))
    (fp_line (start -1.95 3.25) (end 4.5 3.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp abf5169d-db44-434b-a1ea-b76b432688b6))
    (fp_line (start 4.5 -3.25) (end -1.95 -3.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8018a111-a46c-4096-9c71-47a901baa390))
    (fp_line (start 4.5 3.25) (end 4.5 -3.25)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9376b8af-770a-464a-81a5-802a1595b05c))
    (fp_line (start -1.23 -1.469694) (end -1.23 1.469694)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9d06f4bd-efaa-42c3-9708-c84bf3b82b11))
    (fp_arc (start -1.23 -1.469694) (mid 4.17 0.000016) (end -1.230016 1.469666)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 16ca7a8d-8f87-4e62-afc8-457722d6cec7))
    (fp_circle (center 1.27 0) (end 3.77 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 8c57b2be-de86-473e-814e-bd9b215900ae))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(BT1--)") (pinfunction "K") (pintype "passive") (tstamp fbf17069-0445-4da3-b02a-015453924fdd))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D1-A)") (pinfunction "A") (pintype "passive") (tstamp c565e7ec-464a-418b-99c7-3407d1bb008b))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (segment (start 108.48 62.32) (end 109 61.8) (width 0.25) (layer "F.Cu") (net 1) (tstamp 1039f151-c125-41cb-a64d-9fe1447f5f72))
  (segment (start 98.4075 62.32) (end 108.48 62.32) (width 0.25) (layer "F.Cu") (net 1) (tstamp 56467fce-198b-4139-9dea-21614dc24a7d))
  (segment (start 116 78) (end 111 73) (width 0.25) (layer "F.Cu") (net 7) (tstamp 465fd07d-debe-4b74-a277-8d9c9a0beebd))
  (segment (start 117 78) (end 116 78) (width 0.25) (layer "F.Cu") (net 7) (tstamp d0beab42-4849-40d5-945b-726c83b4ffee))
  (segment (start 144.225 65.775) (end 145.5 67.05) (width 0.25) (layer "F.Cu") (net 8) (tstamp 092000df-c3c7-4a0e-8395-3fc679511360))
  (segment (start 127.225 65.775) (end 144.225 65.775) (width 0.25) (layer "F.Cu") (net 8) (tstamp 0ffeaac5-5327-42b8-a3a6-398396ed1fbe))
  (segment (start 117 66.409009) (end 117 70.38) (width 0.25) (layer "F.Cu") (net 8) (tstamp 2ce97346-5424-4e91-8738-475c3a946ece))
  (segment (start 111.5 61.8) (end 112.390991 61.8) (width 0.25) (layer "F.Cu") (net 8) (tstamp 3ebaf1bf-96ae-43d7-ac86-9488ec0c07bb))
  (segment (start 126 67) (end 117.590991 67) (width 0.25) (layer "F.Cu") (net 8) (tstamp 88cb2cb3-151b-4b07-a5de-04797b2aee6a))
  (segment (start 117.590991 67) (end 117 66.409009) (width 0.25) (layer "F.Cu") (net 8) (tstamp 9d5bf484-1234-4e30-a4a4-b9a807abfa52))
  (segment (start 112.390991 61.8) (end 117 66.409009) (width 0.25) (layer "F.Cu") (net 8) (tstamp a232fc75-10c6-4d86-99ee-dfff46076784))
  (segment (start 126 67) (end 127.225 65.775) (width 0.25) (layer "F.Cu") (net 8) (tstamp dca75627-9f2c-4e8a-a2d1-681bc59e090d))

)
